(export (version D)
  (design
    (source /home/cnlohr/electrical/esp_onelayer/esp12e-generics.sch)
    (date "Fri 19 Feb 2016 06:42:15 PM EST")
    (tool "eeschema (2013-jul-07)-stable"))
  (components
    (comp (ref ESP1)
      (value ESP12E)
      (footprint ESP12E)
      (libsource (lib esp12e) (part ESP12E))
      (sheetpath (names /) (tstamps /))
      (tstamp 5619493D))
    (comp (ref U1)
      (value AP1117)
      (footprint SOT223)
      (libsource (lib avr_usb_3v3-cache) (part AP1117))
      (sheetpath (names /) (tstamps /))
      (tstamp 5619494C))
    (comp (ref P1)
      (value CONN_8)
      (footprint SIL-8)
      (libsource (lib conn) (part CONN_8))
      (sheetpath (names /) (tstamps /))
      (tstamp 56194CDB))
    (comp (ref U2)
      (value EXB-A)
      (footprint EXB-A)
      (libsource (lib exb-a) (part EXB-A))
      (sheetpath (names /) (tstamps /))
      (tstamp 56194CEA))
    (comp (ref C1)
      (value 10u)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 56194F36))
    (comp (ref C2)
      (value 10u)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 56194F45)))
  (libparts
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_8)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_8))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))))
    (libpart (lib esp12e) (part ESP12E)
      (fields
        (field (name Reference) ESP)
        (field (name Value) ESP12E)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name REST) (type input))
        (pin (num 2) (name ADC) (type input))
        (pin (num 3) (name CH_PD) (type input))
        (pin (num 4) (name GPIO16) (type input))
        (pin (num 5) (name GPIO14) (type input))
        (pin (num 6) (name GPIO12) (type input))
        (pin (num 7) (name GPIO13) (type input))
        (pin (num 8) (name VCC) (type input))
        (pin (num 9) (name MTDO) (type input))
        (pin (num 10) (name MTDI) (type input))
        (pin (num 11) (name SD_3) (type input))
        (pin (num 12) (name MTMS) (type input))
        (pin (num 13) (name MTCK) (type input))
        (pin (num 14) (name SD_2) (type input))
        (pin (num 15) (name GND) (type input))
        (pin (num 16) (name GPIO15) (type input))
        (pin (num 17) (name GPIO2) (type input))
        (pin (num 18) (name GPIO0) (type input))
        (pin (num 19) (name GPIO4) (type input))
        (pin (num 20) (name GPIO5) (type input))
        (pin (num 21) (name RXD) (type input))
        (pin (num 22) (name TXD) (type input))))
    (libpart (lib avr_usb_3v3-cache) (part AP1117)
      (fields
        (field (name Reference) U)
        (field (name Value) AP1117))
      (pins
        (pin (num 1) (name GND) (type BiDi))
        (pin (num 2) (name Vout) (type BiDi))
        (pin (num 3) (name Vin) (type BiDi))
        (pin (num 4) (name Vout2) (type BiDi))))
    (libpart (lib exb-a) (part EXB-A)
      (fields
        (field (name Reference) U)
        (field (name Value) EXB-A))
      (pins
        (pin (num 1) (name R1) (type BiDi))
        (pin (num 2) (name R2) (type BiDi))
        (pin (num 3) (name R3) (type BiDi))
        (pin (num 4) (name R4) (type BiDi))
        (pin (num 5) (name C) (type BiDi))
        (pin (num 6) (name R5) (type BiDi))
        (pin (num 7) (name R6) (type BiDi))
        (pin (num 8) (name R7) (type BiDi))
        (pin (num 9) (name R8) (type BiDi))
        (pin (num 10) (name C) (type BiDi)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical esp12e)
      (uri /home/cnlohr/electrical/kicad/esp12e.lib))
    (library (logical avr_usb_3v3-cache)
      (uri /home/cnlohr/electrical/kicad/avr_usb_3v3-cache.lib))
    (library (logical exb-a)
      (uri /home/cnlohr/electrical/kicad/exb-a.lib)))
  (nets
    (net (code 1) (name +3.3V)
      (node (ref U1) (pin 2))
      (node (ref ESP1) (pin 3))
      (node (ref ESP1) (pin 8))
      (node (ref ESP1) (pin 1))
      (node (ref C2) (pin 1)))
    (net (code 2) (name GND)
      (node (ref ESP1) (pin 16))
      (node (ref U1) (pin 1))
      (node (ref ESP1) (pin 15))
      (node (ref P1) (pin 7))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2)))
    (net (code 3) (name "")
      (node (ref U2) (pin 5))
      (node (ref U1) (pin 4)))
    (net (code 4) (name +5V)
      (node (ref C1) (pin 1))
      (node (ref P1) (pin 8))
      (node (ref U1) (pin 3)))
    (net (code 5) (name GPIO2)
      (node (ref U2) (pin 4))
      (node (ref U2) (pin 6))
      (node (ref P1) (pin 6))
      (node (ref ESP1) (pin 17)))
    (net (code 6) (name RX)
      (node (ref P1) (pin 2))
      (node (ref ESP1) (pin 21)))
    (net (code 7) (name TX)
      (node (ref ESP1) (pin 22))
      (node (ref P1) (pin 1)))
    (net (code 8) (name GPIO0)
      (node (ref U2) (pin 7))
      (node (ref U2) (pin 3))
      (node (ref P1) (pin 5))
      (node (ref ESP1) (pin 18)))
    (net (code 9) (name GPIO4)
      (node (ref U2) (pin 8))
      (node (ref U2) (pin 2))
      (node (ref ESP1) (pin 19))
      (node (ref P1) (pin 4)))
    (net (code 10) (name GPIO5)
      (node (ref P1) (pin 3))
      (node (ref U2) (pin 1))
      (node (ref U2) (pin 9))
      (node (ref ESP1) (pin 20)))
    (net (code 11) (name "")
      (node (ref ESP1) (pin 10)))
    (net (code 12) (name "")
      (node (ref ESP1) (pin 2)))
    (net (code 13) (name "")
      (node (ref ESP1) (pin 4)))
    (net (code 14) (name "")
      (node (ref ESP1) (pin 5)))
    (net (code 15) (name "")
      (node (ref ESP1) (pin 6)))
    (net (code 16) (name "")
      (node (ref ESP1) (pin 7)))
    (net (code 17) (name "")
      (node (ref ESP1) (pin 9)))
    (net (code 18) (name "")
      (node (ref ESP1) (pin 11)))
    (net (code 19) (name "")
      (node (ref ESP1) (pin 12)))
    (net (code 20) (name "")
      (node (ref ESP1) (pin 13)))
    (net (code 21) (name "")
      (node (ref ESP1) (pin 14)))
    (net (code 22) (name "")
      (node (ref U2) (pin 10)))))