(export (version D)
  (design
    (source /home/cnlohr/electrical/esp_onelayer/esp_onelayer3.sch)
    (date "Wed 02 Sep 2015 04:12:05 PM EDT")
    (tool "eeschema (2013-jul-07)-stable"))
  (components
    (comp (ref X1)
      (value 26MHz)
      (footprint XTAL4P)
      (libsource (lib esp_onelayer2-cache) (part XTAL4P))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8B716))
    (comp (ref U3)
      (value W25Q16DV)
      (footprint SO8ESKINNY)
      (libsource (lib esp_onelayer2-cache) (part 25Q40B))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8B733))
    (comp (ref C5)
      (value 5.6p)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8B75E))
    (comp (ref R4)
      (value 12k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8B7AB))
    (comp (ref R5)
      (value 12k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8B7BD))
    (comp (ref P4)
      (value GND)
      (footprint .1SMTPIN)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8B809))
    (comp (ref P5)
      (value 5V)
      (footprint .1SMTPIN)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8B835))
    (comp (ref P3)
      (value GND)
      (footprint .1SMTPIN)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8B83B))
    (comp (ref C6)
      (value 12p)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8B88E))
    (comp (ref C7)
      (value 12p)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8B894))
    (comp (ref P8)
      (value GPIO0)
      (footprint .1SMTPIN)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8B8D4))
    (comp (ref P7)
      (value UTX)
      (footprint .1SMTPIN)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8B8E6))
    (comp (ref P9)
      (value URX)
      (footprint .1SMTPIN)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8B8EC))
    (comp (ref P6)
      (value GPIO2)
      (footprint .1SMTPIN)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8B90A))
    (comp (ref U1)
      (value AP1117)
      (footprint SOT223)
      (libsource (lib esp_onelayer2-cache) (part AP1117))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8C2C5))
    (comp (ref C3)
      (value 10u)
      (footprint SM0805)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8C2DE))
    (comp (ref C2)
      (value 10u)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8C2E4))
    (comp (ref C1)
      (value 1u)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8C2EA))
    (comp (ref P11)
      (value 5V)
      (footprint .1SMTPIN)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8C79F))
    (comp (ref P10)
      (value GND)
      (footprint .1SMTPIN)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8C838))
    (comp (ref R6)
      (value 0)
      (footprint SM0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8CBA7))
    (comp (ref P12)
      (value GPIO14)
      (footprint .1SMTPIN)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8F0BE))
    (comp (ref P13)
      (value GPIO12)
      (footprint .1SMTPIN)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8F0C4))
    (comp (ref P14)
      (value GPIO5)
      (footprint .1SMTPIN)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8F0CA))
    (comp (ref P16)
      (value GND)
      (footprint .1SMTPIN)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CA0893))
    (comp (ref P17)
      (value GPIO15)
      (footprint .1SMTPIN)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55D24760))
    (comp (ref U2)
      (value ESP8266EX)
      (footprint QFN32)
      (libsource (lib esp_onelayer2-cache) (part ESP8266EX))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8B6FD))
    (comp (ref C8)
      (value .1u)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 55E475A5))
    (comp (ref P2)
      (value UFL)
      (footprint UFL)
      (libsource (lib conn) (part CONN_2))
      (sheetpath (names /) (tstamps /))
      (tstamp 55E474E2))
    (comp (ref P1)
      (value MIC)
      (footprint .1SMTPIN)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55C8B86A))
    (comp (ref R2)
      (value NP)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55E48F87))
    (comp (ref R1)
      (value 333k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55E48F8D))
    (comp (ref R3)
      (value 12k)
      (footprint SM0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55E49550))
    (comp (ref R7)
      (value 0)
      (footprint SM0805)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55E49C42))
    (comp (ref C4)
      (value 10u)
      (footprint SM0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 55E70B25))
    (comp (ref P15)
      (value 5V)
      (footprint .1SMTPIN)
      (libsource (lib conn) (part CONN_1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55E75812)))
  (libparts
    (libpart (lib device) (part C)
      (description "Condensateur non polarise")
      (footprints
        (fp SM*)
        (fp C?)
        (fp C1-1))
      (fields
        (field (name Reference) C)
        (field (name Value) C)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part R)
      (description Resistance)
      (footprints
        (fp R?)
        (fp SM0603)
        (fp SM0805)
        (fp R?-*)
        (fp SM1206))
      (fields
        (field (name Reference) R)
        (field (name Value) R)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_1)
      (description "1 pin")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_1))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib conn) (part CONN_2)
      (description "Symbole general de connecteur")
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_2))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name PM) (type passive))))
    (libpart (lib esp_onelayer2-cache) (part 25Q40B)
      (fields
        (field (name Reference) U)
        (field (name Value) 25Q40B)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name ~CS) (type input))
        (pin (num 2) (name DO/IO1) (type input))
        (pin (num 3) (name ~WP~/IO2) (type input))
        (pin (num 4) (name GND) (type input))
        (pin (num 5) (name DI/IO0) (type input))
        (pin (num 6) (name CLK) (type input))
        (pin (num 7) (name ~HOLD~/IO3) (type input))
        (pin (num 8) (name VCC) (type input))
        (pin (num 9) (name GND) (type input))))
    (libpart (lib esp_onelayer2-cache) (part AP1117)
      (fields
        (field (name Reference) U)
        (field (name Value) AP1117)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name GND) (type BiDi))
        (pin (num 2) (name Vout) (type BiDi))
        (pin (num 3) (name Vin) (type BiDi))
        (pin (num 4) (name Vout2) (type BiDi))))
    (libpart (lib esp_onelayer2-cache) (part ESP8266EX)
      (fields
        (field (name Reference) U)
        (field (name Value) ESP8266EX)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name VddA) (type input))
        (pin (num 2) (name LNA/ANT) (type input))
        (pin (num 3) (name Vdd3P3) (type input))
        (pin (num 4) (name Vdd3P3) (type input))
        (pin (num 5) (name VddRCT) (type input))
        (pin (num 6) (name TOUT) (type input))
        (pin (num 7) (name CHIP_EN) (type input))
        (pin (num 8) (name XPD_DCDC) (type input))
        (pin (num 9) (name MTMS/GPIO14) (type input))
        (pin (num 10) (name MTDI/GPIO12) (type input))
        (pin (num 11) (name VddPST) (type input))
        (pin (num 12) (name MTCK/GPIO13) (type input))
        (pin (num 13) (name MTDO/GPIO15) (type input))
        (pin (num 14) (name GPIO2) (type input))
        (pin (num 15) (name GPIO0) (type input))
        (pin (num 16) (name GP4/VD) (type input))
        (pin (num 17) (name VddPST) (type input))
        (pin (num 18) (name SD_D2) (type input))
        (pin (num 19) (name SD_D3) (type input))
        (pin (num 20) (name SD_CMD) (type input))
        (pin (num 21) (name SD_CLK) (type input))
        (pin (num 22) (name SD_D0) (type input))
        (pin (num 23) (name SD_D1) (type input))
        (pin (num 24) (name GP5/VD) (type input))
        (pin (num 25) (name URXD) (type input))
        (pin (num 26) (name UTXD) (type input))
        (pin (num 27) (name XTAL_OUT) (type input))
        (pin (num 28) (name XTAL_IN) (type input))
        (pin (num 29) (name VDDD) (type input))
        (pin (num 30) (name VDDA) (type input))
        (pin (num 31) (name RES12K) (type input))
        (pin (num 32) (name EXT_RSTB) (type input))
        (pin (num 33) (name GND) (type input))))
    (libpart (lib esp_onelayer2-cache) (part XTAL4P)
      (fields
        (field (name Reference) X)
        (field (name Value) XTAL4P)
        (field (name Footprint) ~)
        (field (name Datasheet) ~))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name GND) (type passive))
        (pin (num 4) (name GND) (type passive)))))
  (libraries
    (library (logical device)
      (uri /usr/share/kicad/library/device.lib))
    (library (logical conn)
      (uri /usr/share/kicad/library/conn.lib))
    (library (logical esp_onelayer2-cache)
      (uri /home/cnlohr/electrical/esp_onelayer/esp_onelayer2-cache.lib)))
  (nets
    (net (code 1) (name "")
      (node (ref U2) (pin 16))
      (node (ref P14) (pin 1)))
    (net (code 2) (name "")
      (node (ref U2) (pin 9))
      (node (ref P12) (pin 1)))
    (net (code 3) (name "")
      (node (ref U2) (pin 10))
      (node (ref P13) (pin 1)))
    (net (code 4) (name "")
      (node (ref U2) (pin 18))
      (node (ref R6) (pin 1)))
    (net (code 5) (name "")
      (node (ref U2) (pin 26))
      (node (ref P7) (pin 1)))
    (net (code 6) (name "")
      (node (ref U2) (pin 5)))
    (net (code 7) (name "")
      (node (ref U2) (pin 21))
      (node (ref U3) (pin 6)))
    (net (code 8) (name "")
      (node (ref U2) (pin 23))
      (node (ref U3) (pin 5)))
    (net (code 9) (name "")
      (node (ref U3) (pin 2))
      (node (ref U2) (pin 22)))
    (net (code 10) (name "")
      (node (ref U2) (pin 20))
      (node (ref U3) (pin 1)))
    (net (code 11) (name "")
      (node (ref U3) (pin 3))
      (node (ref U2) (pin 19)))
    (net (code 12) (name "")
      (node (ref R6) (pin 2))
      (node (ref U3) (pin 7)))
    (net (code 13) (name +5V)
      (node (ref P15) (pin 1))
      (node (ref C3) (pin 2))
      (node (ref U1) (pin 3))
      (node (ref P11) (pin 1)))
    (net (code 14) (name GND)
      (node (ref C3) (pin 1))
      (node (ref P16) (pin 1))
      (node (ref U1) (pin 1))
      (node (ref P2) (pin 2))
      (node (ref R2) (pin 1))
      (node (ref U2) (pin 33))
      (node (ref U2) (pin 24))
      (node (ref X1) (pin 4))
      (node (ref X1) (pin 3))
      (node (ref C7) (pin 2))
      (node (ref U3) (pin 4))
      (node (ref C6) (pin 2))
      (node (ref P3) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref P4) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref P10) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref R3) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref U2) (pin 8))
      (node (ref U2) (pin 12))
      (node (ref C8) (pin 1))
      (node (ref C4) (pin 1)))
    (net (code 15) (name "")
      (node (ref R3) (pin 1))
      (node (ref P17) (pin 1))
      (node (ref U2) (pin 13)))
    (net (code 16) (name "")
      (node (ref R1) (pin 2))
      (node (ref U2) (pin 6))
      (node (ref R2) (pin 2))
      (node (ref P1) (pin 1)))
    (net (code 17) (name +3.3V)
      (node (ref C8) (pin 2))
      (node (ref U2) (pin 4))
      (node (ref U2) (pin 1))
      (node (ref U2) (pin 32))
      (node (ref U2) (pin 11))
      (node (ref U2) (pin 30))
      (node (ref U2) (pin 29))
      (node (ref R1) (pin 1))
      (node (ref U2) (pin 7))
      (node (ref U2) (pin 3))
      (node (ref C4) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref U1) (pin 4))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref U1) (pin 2))
      (node (ref P5) (pin 1))
      (node (ref U2) (pin 17))
      (node (ref U3) (pin 8)))
    (net (code 18) (name "")
      (node (ref P8) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref U2) (pin 15)))
    (net (code 19) (name "")
      (node (ref U2) (pin 31))
      (node (ref R4) (pin 2)))
    (net (code 20) (name "")
      (node (ref C5) (pin 2))
      (node (ref U2) (pin 2)))
    (net (code 21) (name "")
      (node (ref C5) (pin 1))
      (node (ref P2) (pin 1)))
    (net (code 22) (name "")
      (node (ref U3) (pin 9)))
    (net (code 23) (name "")
      (node (ref P6) (pin 1))
      (node (ref U2) (pin 14)))
    (net (code 24) (name "")
      (node (ref U2) (pin 25))
      (node (ref P9) (pin 1)))
    (net (code 25) (name "")
      (node (ref U2) (pin 27))
      (node (ref C7) (pin 1))
      (node (ref X1) (pin 1)))
    (net (code 26) (name "")
      (node (ref C6) (pin 1))
      (node (ref X1) (pin 2))
      (node (ref U2) (pin 28)))))